INBNGEO    PART5.geo                                                            &   Input binary geometry file                                                                                                                        
INELEV     2014-10.TID                                                          &   Input time series of elevation file                                                                                                               
INELTFL    est-10B.elf                                                          &   Input time series of element inflow data                                                                                                          
OUTFIL     ESTDYN10B.OUT                                                        &   Output ASCII results file                                                                                                                         
OUTBNRMA   ESTDYN10B.RMA                                                        &   Output binary results file                                                                                                                        
OUTBNRST   ESTDYN10B.RST                                                        &   Output binary restart file                                                                                                                        
ENDFIL                                                                                                                                                                                                                                
ENDLIMIT                                                                                                                                                                                                                              
TI                                                                Ralphs Bay                                                                                                                                                          
STARTIM    01/08/2014 00.00                                          $ Starting date and time                                                                                                                                         
ENDTIM                                                               $ Ending date and time                                                                                                                                           
VERTTURB       1                                                     $ Vertical turbulence option                                                                                                                                     
MARSHOPT      -2                                                     $ Marsh option 0=inactive -2 = input marsh parameters                                                                                                            
EDDYTYPE       1                                                     $ Eddy type 0 = fixed, 1= scaled, 2 =  Smagorinsky                                                                                                               
TBFACT     0.200                                                     $ Turbulence factor when Smagorinsky is active                                                                                                                   
TBMINT     2.000                                                     $ Turbulence minimum when Smagorinsky is active                                                                                                                  
TIMPROJ        1                                                     $ Time projection switch 1= no projection, 0 = use time derivative (least stable), 2 = project u                                                                 
3DTYPLD3                                                             $ 3-d model with type LD3 input                                                                                                                                  
GRAVITY        1                                                     $ Units switch   1 = metric    0 = english                                                                                                                       
ZEROBED        0                                                     $ Force zero bed velocity 1 = at all bed levels   2 = limited by bed level input                                                                                 
ZERBELLV   0.000                                                     $ Force zero velocity on water surface                                                                                                                           
PASSSAL        0                                                     $ Bed level below which zero bed level in applied                                                                                                                
PASSTMP        0                                                     $ Ignore influence of salinity on water density                                                                                                                  
PASSSED        0                                                     $ Ignore influence of temperature on water density                                                                                                               
ZEROSURF       0                                                     $ Ignore influence of sediment on water density                                                                                                                  
SAVITR       0                                                       $ Save binary file for all iterations 0 = ignore,  1 =save                                                                                                       
REVRTDEN   0.000                                                     $ Option for vertical density model   0 = standard  1 = revised method                                                                                           
OMEGA    -42.900                                                     $ Latitude (degrees) positive in northern hemisphere                                                                                                             
ELEV       0.500                                                     $ Reference level for vertical transformation / Starting water level                                                                                             
X-SCALE    0.000                                                     $ x scale factor  (0.0 equivalent to 1.0)                                                                                                                        
Y-SCALE    0.000                                                     $ y scale factor  (0.0 equivalent to 1.0)                                                                                                                        
Z-SCALE    0.000                                                     $ z sacle factor  (0.0 equivalent to 1.0)                                                                                                                        
TRNSCVAL   0.000                                                                                                                                                                                                                      
TRNSPOWR   0.000                                                                                                                                                                                                                      
UNOM       0.000                                                                                                                                                                                                                      
UDIR       0.000                                                                                                                                                                                                                      
HMIN       0.000                                                                                                                                                                                                                      
DSET       0.000                                                                                                                                                                                                                      
DSETD      0.000                                                                                                                                                                                                                      
FIXBC          0                                                                                                                                                                                                                      
VERTEQSW       0                                                                                                                                                                                                                      
INITSAL   35.000                                                                                                                                                                                                                      
INITTEMP  20.000                                                                                                                                                                                                                      
INITSED    0.000                                                                                                                                                                                                                      
INITUBED   0.000                                                                                                                                                                                                                      
INITVBED   0.000                                                                                                                                                                                                                      
RETRNPCT   0.000                                                                                                                                                                                                                      
SURFMIX    0.500                                                                                                                                                                                                                      
SSITN          0                                                                                                                                                                                                                      
TRITN          6                                                                                                                                                                                                                      
TRSTEPS       96                                                                                                                                                                                                                      
TRITN          0                                                                                                                                                                                                                      
ASCSVFRQ      10                                                                                                                                                                                                                      
STBIN          0                                                                                                                                                                                                                      
DRYSW          0                                                                                                                                                                                                                      
FRQBIN         0                                                                                                                                                                                                                      
FRQRST        40                                                                                                                                                                                                                      
RWASCFRQ       0                                                                                                                                                                                                                      
1DTYP          0                                                                                                                                                                                                                      
SOLVER         4                                                                                                                                                                                                                      
SLVERDSK       0                                                                                                                                                                                                                      
MESSRWND       0                                                                                                                                                                                                                      
INITWSRF   0.000                                                                                                                                                                                                                      
CONV-VEL 0.00100                                                                                                                                                                                                                      
CONV-DEP 0.00010                                                                                                                                                                                                                      
CONV-SAL 0.00300                                                                                                                                                                                                                      
CONV-TMP 0.00000                                                                                                                                                                                                                      
CONV-SED 0.00000                                                                                                                                                                                                                      
EDDY-MAT       1  -0.20000                                                                                                                                                                                                            
EDDY-VRT       1   0.10000                                                                                                                                                                                                            
DIFF-MAT       1   0.10000                                                                                                                                                                                                            
DIFF-VRT       1   0.02500                                                                                                                                                                                                            
MANN-MAT       1   0.04000                                                                                                                                                                                                            
MANN-BNK       1   0.02000                                                                                                                                                                                                            
MANN-SRF       1   0.00000                                                                                                                                                                                                            
MARSH-FR       1  25.00000                                                                                                                                                                                                            
ED-VTVAR       1   1.000   0.000   0.000                                                                                                                                                                                              
BN-V-MIN   1.000                                                                                                                                                                                                                      
BN-V-PWR   1.000                                                                                                                                                                                                                      
TR-V-MIN   1.000                                                                                                                                                                                                                      
TR-V-PWR   1.000                                                                                                                                                                                                                      
LD3            0       4  -1.000  -3.500  -7.000 -50.000                                                                                                                                                                              
MARSH-SH   2.000                                                                                                                                                                                                                      
MARSH-SH   0.500                                                                                                                                                                                                                      
MARSH-PR   0.010                                                                                                                                                                                                                      
MARSH-LM   0.000                                                                                                                                                                                                                      
TAB-END                                                                                                                                                                                                                               
ENDGEO                                                                                                                                                                                                                                
DELTA-HR      0.0000                                                 & Time step in minutes                                                                                                                                           
QSL-ITR                                                              & iterate on flow/depth and salinity -2- flow/depth and -1- salinty iterations per cycle                                                                         
FL-ELEVC       1       0  0.5000  35.000  20.000   0.000             & Continuity line elevation FL-ELEVC is elevation specified as constant along a line (subs values from file)- CCLINE, Elevation ,bc-sal,bc-temp,bc-sed           
FL-ELMET     584       0 50.0000   5.000  20.000   0.000             & Element Inflow listing element number and total inflow into element.  Elt num, Lay num,flow rate,salinity,temp,sediment -FL means subsequent values from file  
CN-ELMET     585       0 51.0000   6.000  21.000   1.000             & Element Inflow listing element number and total inflow into element.  Elt num, Lay num,flow rate,salinity,temp,sediment -FL means subsequent values from file  
CN-ELMED     586       1  2.0000   7.000  22.000   2.000             & Element Inflow listing element number and spec flow into element. Elt num, Lay num,flow rate,salinity,temp,sediment -FL means subsequent values from file      
CN-ELMGD       1  3.0000   8.000  23.000   3.000                     & Element Inflow  treated as a total rate over all given layer of elements. Lay num,flow rate,salinity,temp,sediment -FL means subsequent values from file       
CN-ELMGT       2 52.0000   9.000  24.000   4.000                     & Element Inflow  treated as a spcific rate over all given layer of elements. Lay num,flow rate,salinity,temp,sediment -FL means subsequent values from file     
CN-RAIN   4.0000  10.000  25.000   5.000                             & Element Inflow  treated as a rainfall rate (in mm/day) over all surface elementa. flow rate,salinity,temp,sediment -FL means subsequent values from file       
CN-GRAIN       1  5.0000  11.000  26.000   6.000                     & Element Inflow listing element inflow for a given group and rainfall into element. Grp num,flow rate,salinity,temp,sed -FL means subsequent values from file   
DELTA-HR      0.2500                                                 & Time step in minutes                                                                                                                                           
DATE-END    31/12/2014 00.00                                         & Ending time for the time step block                                                                                                                            
QSL-ITR                                                              & iterate on flow/depth and salinity -2- flow/depth and -1- salinty iterations per cycle                                                                         
ENDSTEP                                                                                                                                                                                                                               
ENDDATA                                                                                                                                                                                                                               
